### **A Literature Survey Smart Farmer - IoT Enabled Smart Farming Application**

**ABSTACTION:**

India is agriculture sector, on either side, is losing ground every day, affecting the ecosystem\'s output capacity. In order to restore vitality and put agriculture back on a path of higher growth, there is a growing need to resolve the issue. A large-scale agricultural system necessitates a great deal of upkeep, knowledge, and oversight. The IoT is a network of interconnected devices that can transmit and receive data over the internet and carry out tasks without human involvement. Agriculture provides a wealth of data analysis parameters, resulting in increased crop yields. The use of IoT devices in smart farming aids in the modernization of information and communication. For better crop growth moisture, mineral, light and other factors can be assumed. This research looks into a few of these characteristics for data analysis with the goal of assisting users in making better agricultural decisions using IoT . The technique is intended to help farmers increase their agricultural output.

**Introduction :**

The India is an agricultural country.  Nowadays, at regular intervals the lands are manually irrigated by the farmers. There is a chance that the water consumption will be higher or that the time it takes for the water to reach the destination will be longer, resulting in crop dryness. Real-time temperature and humidity monitoring is crucial in many agricultural disciplines. However, the old method of wired detection control is inflexible, resulting in several application limitations. This project achieves irrigation automation as a crucial answer to this problem. This is accomplished with the aid of a Raspberry Pi, which controls the moisture and temperature sensors based on the input provided. Moisture sensors are used in the construction of an automated plant watering system for this purpose. The main aim of our project is to reduce the complexity of supervision and to avoid the continuous monitoring. We can accomplish smart agriculture using our system. This system includes IoT-based agricultural monitoring. The Internet of Things (IOT) is transforming the agriculture business and addressing the enormous difficulties and huge obstacles that farmers confront today in the field. The soil moisture sensor is put into the soil to determine whether the soil is wet or dry, and If the moisture level in the soil is low, the relay unit attached to the motor switch must be monitored on a regular basis. When the soil is dry, it will turn on the motor, and when the soil is moist, it will turn off the engine.

**LITERATURE REVIEW :**

The term "Internet of Things" refers to the connection of objects, equipment, vehicles, and other electronic devices to a network for the purpose of data exchange (IoT). The Internet of Things (IoT) is increasingly being utilised to connect objects and collect data. As a result, the Internet of Things' use in agriculture is crucial. The idea behind the project is to create a smart agriculture system that is connected to the internet of things. The technology is combined with an irrigation system to deal with Malaysia's variable weather. This system's microcontroller is a Raspberry Pi 4 Model B. The temperature and humidity in the surrounding region, as well as the moisture level of the soil, are monitored using the DHT22 and soil moisture sensor. The data will be available on both a smartphone and a computer.  As a result, Internet of Things (IoT) and Raspberry Pi-based Smart Agriculture Systems have a significant impact on how farmers work. It will have a good impact on agricultural productivity as well. In Malaysia, employing IoT-based irrigation systems saves roughly 24.44 percent per year when compared to traditional irrigation systems. This would save money on labour expenditures while also preventing water waste in daily needs.

##### **Conclusion :**

##### Conclude The proposed work provides the information on various soil parameters that includes soil temperature, soil moisture and atmospheric temperature to predict irrigation suitability. This system helps to analyze the soil parameters thereby ensuring a better system of irrigation for agriculture. The data collected from the sensors are made to learn using machine learning techniques to ensure a fully automated sys- tem. Implementing an IoT based smart agriculture system helps in obtaining quality crops and it also reduces the human involvement in agricultural activities.

##### **References :**

[1] Zuraida Muhammad,Muhammad Azri Asyraf Mohd Hafez,Nor Adni Mat”Smart Agriculture Using Internet of Things with Raspberry Pi.” 2020.

[2] Divya J., Divya M.,Janani V.”IoT based Smart Soil Monitoring System for Agricultural Production” 2017.

[3] H.G.C.R.Laksiri, H.A.C.Dharmagunawardhana, J.V.Wijayakulasooriya ”Design and Optimization of loT Based Smart Irrigation System in Sri Lanka”2019

[4] Anushree Math, Layak Ali, Pruthviraj U ”Development of Smart Drip Irriga- tion System Using IoT”2018.